{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"sheet1","index":0,"n_rows":38,"n_cols":12,"rows_kept":38,"cut":false,"hidden":false,"merged":[[0,0,0,11],[1,0,1,11],[2,0,2,11]]}
["정산요소 내역"]
["조회기간 : 2020-04-01 ~ 2020-04-30"]
["단위 : MWh"]
["연료원코드","연료원","설비용량(MW)","A","RA","ARA","MGO","AMGO","PSE","FCA","OFCA","OR"]
[1,"원자력",23250,13122533,13056626,13056588.200999999,13049335.517526001,13049335.517526001,13119385,13057831.991386,13056626,0]
[2,"유연탄",36906.281999999999,16077356,15947236,15945913.211999999,13993560.048684999,13993546.841484999,15811588,15947371.219439,15947236,0]
[3,"무연탄",600,130307,130307,130307,116449.86798,116449.86798,110942,130343.553671,130307,0]
[5,"바이오가스",81.622,0,0,0,33483.908624000003,33483.908624000003,0,0,0,0]
[6,"부생가스",4243.47,0,0,0,519226.21450599999,519226.21450599999,0,0,0,0]
[7,"소수력",192.09,0,0,0,40856.502117000004,40856.502117000004,0,0,0,0]
[8,"수력",1604.98,164445,164091,164091,169253.145911,169253.145911,164387,0,0,0]
[9,"양수",4700,1450,1450,1450,296284.643056,296284.643056,-1979,0,0,0]
[10,"매립가스",66.147999999999996,0,0,0,12337.008954000001,12337.008954000001,0,0,0,0]
[12,"중유",1558.3,714499,705230,705226.76800000004,111727.31322900001,111727.31322900001,8466,705230.07956400001,705230,0]
[13,"태양광",3755.5650000000001,0,0,0,570929.52770199999,570929.52770199999,0,0,0,0]
[15,"폐기물",327.68200000000002,0,0,0,91704.167323000001,91704.167323000001,0,0,0,0]
[16,"풍력",1562.173,0,0,0,309315.10871599999,309315.10871599999,0,0,0,0]
[17,"LNG",40296.086000000003,26075641,25725070,25720293.754000001,9012993.7668890003,9012993.7668890003,6771019,25728362.379232001,25724909,233252]
[20,"연료전지",530.53,0,0,0,252038.055077,252038.055077,0,0,0,0]
[21,"경유",465.8,354633,355052,355052,0,0,0,355052,355052,0]
[22,"해양에너지",255.5,0,0,0,37814.336592,37814.336592,0,0,0,0]
[23,"가스압",0.3,0,0,0,0,0,0,0,0,0]
[24,"바이오매스",401.05399999999997,0,0,0,162829.530646,162829.530646,0,0,0,0]
[25,"IGCC",346.33,0,0,0,203736.00072000001,203736.00072000001,0,0,0,0]
[32,"바이오중유",350,243360,243109,243109,129079.353424,129079.353424,22237,243109.33136800001,243109,0]
[40,"RPS",0,0,0,0,0,0,0,0,0,0]
[99,"기타",84.29,0,0,0,52507.816910000001,52507.816910000001,0,0,0,0]
["원자력합","원자력합",23250,13122533,13056626,13056588.200999999,13049335.517525999,13049335.517525999,13119385,13057831.991386,13056626,0]
["석탄합","석탄합",37506.281999999999,16207663,16077543,16076220.211999999,14110009.916664999,14109996.709464999,15922530,16077714.773110004,16077543,0]
["LNG합","LNG합",40296.086000000003,26075641,25725070,25720293.754000001,9012993.7668890003,9012993.7668890003,6771019,25728362.379232001,25724909,233252]
["유류합","유류합",2024.1,1069132,1060282,1060278.7679999999,111727.31322899998,111727.31322899998,8466,1060282.079564,1060282,0]
["양수합","양수합",4700,1450,1450,1450,296284.643056,296284.643056,-1979,0,0,0]
["신재생합","신재생합",13717.144,407805,407200,407200,2532602.860311999,2532602.860311999,186624,243109.33136799998,243109,0]
["기타합","기타합",84.59,0,0,0,52507.816910000001,52507.816910000001,0,0,0,0]
["수력합","수력합",1797.07,164445,164091,164091,210109.648028,210109.648028,164387,0,0,0]
["폐기물합","폐기물합",4571.152,0,0,0,610930.38182899985,610930.38182899985,0,0,0,0]
["바이오합","바이오합",898.82399999999996,243360,243109,243109,337729.80164800002,337729.80164800002,22237,243109.33136799998,243109,0]
["총계",null,121578.202,56884224,56328171,56322030.935000002,39165461.834587,39165448.627387002,36006045,56167300.55466,56162469,233252]